#N canvas 3 0 513 348 12;
#X obj 66 15 delay;
#X obj 13 229 50;
#X msg 13 98 bang;
#X floatatom 13 255;
#X floatatom 116 182;
#X obj 51 230 0;
#X text 111 16 - CALLBACK AFTER TIME DELAY;
#X text 130 205 <-- creation argument initializes delay time;
#X text 6 41 The delay object sends a bang to its outlet after a delay in milliseconds specified by its right inlet or its creation argument.;
#X obj 51 204 delay 1000;
#X text 58 86 Click here to test the delay object by initializing the number box below to 50 and then clearing it after the specified delay.;
#X text 94 132 Click here to CANCEL delay's action;
#X msg 51 133 stop;
#X text 43 324 see also:;
#X obj 155 323 timer;
#X obj 111 323 metro;
#X msg 62 155 2000;
#X text 102 154 Number in right inlet sets time and schedules the action.;
#X text 316 320 updated for Pd version 0.3;
#X text 145 183 <-- scroll to change delay time in milliseconds;
#X text 14 280 Note: sending a bang to a delay which is already set will reschedule its output \, cancelling the old one.;
#X connect 1 0 3 0;
#X connect 2 0 1 0;
#X connect 2 0 9 0;
#X connect 4 0 9 1;
#X connect 5 0 3 0;
#X connect 9 0 5 0;
#X connect 12 0 9 0;
#X connect 16 0 9 0;
