#N canvas 59 19 612 342 12;
#X obj 35 11 spigot;
#X text 100 12 - pass or block messages;
#X text 35 63 Spigot passes messages from its left inlet to its outlet
\, as long as a nonzero number is sent to its right inlet. When its
right inlet gets zero \, incoming messages are "blocked \, " i.e. \,
ignored.;
#X msg 25 157 0.5 1000;
#X obj 25 300 print;
#X msg 38 210 walk the cat;
#X msg 31 182 bang;
#X text 128 240 control: nonzero to pass messages \, zero to stop them
;
#X obj 25 267 spigot 0;
#X text 349 310 updated for Pd version 0.38;
#X obj 92 244 tgl 15 0 empty empty empty 0 -6 0 8 -262144 -1 -1 0 1
;
#X text 450 267;
#X text 125 267 optional arg sets the initial state (0 by default)
;
#X connect 3 0 8 0;
#X connect 5 0 8 0;
#X connect 6 0 8 0;
#X connect 8 0 4 0;
#X connect 10 0 8 1;
